Text for specification

Description
CRITO®
universal conductor terminal
4 - 35 mm², AWG 12 - 2
30Compact 3P
60Classic
100Energy
185mm-System

Standards
IEC 61439-1:2020
IEC 60999-1:1999
IEC 60999-2:2003

Approvals
CSA, UL

Electrical data
Rated current (IEC):	115 A
rated voltage (IEC) AC:	690 V

rated current (UL):	115 A
rated voltage (UL) AC:	600 V
current capacity (IEC) max.:	270 A
max. permitted voltage (IEC) AC:	1000 V
max. permitted voltage (IEC) DC:	1500 V

rated peak withstand current  Ipk max.:	34.9 kA

Terminal points
4 - 35 mm² / AWG 10 - AWG 2 
flexible cables, directly or with wire-end ferrule, 
solid and stranded round cables, 
lam. Cu 3 x 9 x 0.8 or 6 x 9 x 0.8

(flexible cables of maximum cross-section may not fit when using wire-end ferrule)

Miscellaneous 
Terminal with integrated holding spring, captive clamping screw and opened terminal space.
Indication of nominal cross-section and tightening torque noted on the terminal.

Brand 
Woehner or equivalent

Part No.
01290000