Text for specification

Description
CRITO®
brace terminal
lam. Cu. 20x3 ... 32x15
60Classic
100Energy
185mm-System
centre feed unit

Standards
IEC 61439-1:2011
IEC 60999-1:1999
IEC 60999-2:2003

Approvals
UL

Electrical data
Rated current (IEC):	500 A
rated voltage (IEC) AC:	690 V

rated current (UL):	800 A
rated voltage (UL) AC:	600 V
current carrying capacity for centre feed:	750 A
current capacity (IEC) max.:	750 A
max. permitted voltage (IEC) AC:	1000 V
max. permitted voltage (IEC) DC:	1500 V

SCCR:	25 kA

Terminal points
lam. Cu from 3 x 20 x 1 to 10 x 24 x 1

Miscellaneous 
Terminal with captive clamping screws, conductor can be overlapped, indication of nominal cross-section and tightening torque noted on the terminal. Contact between conductor and busbar via contact block.

Brand 
Woehner or equivalent

Part No.
01319000