Text for specification

Description
universal busbar support
4-pole with internal screw holes
60Classic

Standards
IEC 61439-1:2011

Approvals
CSA, UL

Electrical data
rated voltage (IEC) AC:	800 V
rated voltage (UL) AC:	600 V

rated isolation voltage U_i AC:	1000 V
rated surge voltage U_imp :	8 kV

Kurzschlussfestigkeit:
Siehe Kurzschlussdiagramm im Bereich Download

Miscellaneous 
With internal screw holes
can also be used as centre support
With the 4th pole, the width of the busbar can be set independent of L1, L2 and L3.

Brand 
Woehner or equivalent

Part No.
01485000