Text for specification

Description
AMBUS Panel
holder for cylindrical fuses, with LED
Class CC / 3P
30 A / 600 V

Standards
IEC 60269-1:2006 + A1:2009 + A2:2014
IEC 60269-2:2013 + A1:2016, Fuse system J

Approvals
CSA, UL, CCC

Electrical data

rated current (UL):	30 A
rated voltage (UL) AC:	600 V
rated voltage (UL) DC:	600 V

power dissipation at full load of the item:	0.9 W

SCCR:	200 kA

indicator light
operating voltage range: 110 - 600 V AC / DC

Miscellaneous 
large clamping range, also for two identical conductors (adjacent)
holder for label
with indicator for tripped fuse
any polarity for DC voltage

Brand 
Woehner or equivalent

Part No.
31300000