Text for specification

Description
SECUR®Panel
switch-disconnector for D0 fuses up to 63 A
2P

Standards
IEC 60947-1:2020
IEC 60947-3:2020 AC ratings only

Approvals
VDE, CCC

Electrical data
Rated current (IEC):	63 A
rated voltage (IEC) AC:	400 V
rated voltage (IEC) DC:	130 V

AC-22B (400V)

DC-22B (130 V)

power dissipation at full load of the item:	5.2 W

rated isolation voltage Ui AC:	500 V
rated surge voltage Uimp :	6 kV

for fuse links and gauge rings as per DIN VDE 0636-3 IEC / HD 60269-3
utilisation category as per VDE 0638 : AC-22

Brand 
Woehner or equivalent

Part No.
31313000A