Text for specification

Description
EQUES^®60Classic
busbar adapter 400 A, 3-pole
laminated copper
140 x 320
60Classic

Standards
IEC 61439-1:2011

Electrical data
Rated current (IEC):	400 A
rated voltage (IEC) AC:	690 V

power dissipation at full load of the item:	17.9 W

rated isolation voltage U_i AC:	800 V
rated surge voltage U_imp :	6 kV
max. permitted voltage (IEC) DC:	800 V

rated peak withstand current  I_pk max.:	36 kA

Brand 
Woehner or equivalent

Part No.
32046000B