Text for specification

Description
EQUES^®60Classic
busbar adapter 250 A, 3-pole
105 x 240
60Classic

Standards
IEC 61439-1:2011

Approvals
CSA, UL

Electrical data
Rated current (IEC):	250 A
rated voltage (IEC) AC:	690 V

rated current (UL):	250 A
rated voltage (UL) AC:	600 V

power dissipation at full load of the item:	18.0 W

rated isolation voltage U_i AC:	800 V
rated surge voltage U_imp :	6 kV

SCCR: 35 kA with DIVQ/7 250A / 600 V AC, 100 kA with DIVQ/7 250A / 480 V AC 

Brand 
Woehner or equivalent

Part No.
32050000A