Text for specification

Description
EQUES®60Classic
busbar adapter 250 A, 3-pole
copper tube connection
105 x 200, bottom connection
60Classic

Standards
IEC 61439-1:2011

Electrical data
Rated current (IEC):	250 A
rated voltage (IEC) AC:	690 V

power dissipation at full load of the item:	9.6 W

rated isolation voltage Ui AC:	800 V
rated surge voltage Uimp :	6 kV

Brand 
Woehner or equivalent

Part No.
32052000B