Text for specification

Description
EQUES®60Classic
busbar adapter 200 A
terminals 6 - 70 mm² at bottom
108 x 222
60Classic

Standards
IEC 61439-1:2011

Approvals
CSA, UL

Electrical data
Rated current (IEC):	200 A
rated voltage (IEC) AC:	690 V

rated current (UL):	200 A
rated voltage (UL) AC:	600 V

rated isolation voltage Ui AC:	800 V
rated surge voltage Uimp :	6 kV
max. permitted voltage (IEC) DC:	800 V

rated peak withstand current  Ipk max.:	46.9 kA

Brand 
Woehner or equivalent

Part No.
32215000