Text for specification

Description
EQUES®CrossBoard
adapter 63 A
phase L3, 1 fixed mounting rail, with leads AWG 8 (10 mm²)
18 x 160

Standards
IEC 61439-1:2011

Approvals
UL

Electrical data
Rated current (IEC):	63 A
rated voltage (IEC) AC:	690 V

rated current (UL):	63 A
rated voltage (UL) AC:	600 V

power dissipation at full load of the item:	2.5 W

rated isolation voltage Ui AC:	800 V
rated surge voltage Uimp :	6 kV

rated peak withstand current  Ipk max.:	9.5 kA

SCCR: 10 kA with any DIVQ/7 circuit breaker 63 A / 480 V AC, 65 kA with any 3-pole NKJH/7 Comb. Motor Controller 63 A / 480 V AC, 200 kA with JDDZ fuse Class CC, CF, J, T 60 A / 600 V AC, 65 kA with any 1-pole NKJH/7 Comb. Motor Controller 63 A / 277 V AC 

Brand 
Woehner or equivalent

Part No.
32309000A