Text for specification

Description
EQUES®CrossBoard
component support
without electrical connection, 1 fixed mounting rail
18 x 160

Standards
IEC 61439-1:2011

Approvals
UL

Electrical data
rated voltage (IEC) AC:	690 V

rated isolation voltage Ui AC:	800 V
rated surge voltage Uimp :	6 kV

Brand 
Woehner or equivalent

Part No.
32311000A