Text for specification

Description
EQUES®60Classic
busbar adapter 125 A, 3-pole
90 x 200
60Classic

Standards
IEC 61439-1:2011

Approvals
CSA, UL

Electrical data
Rated current (IEC):	125 A
rated voltage (IEC) AC:	690 V

rated current (UL):	125 A
rated voltage (UL) AC:	600 V

power dissipation at full load of the item:	12.0 W

rated isolation voltage Ui AC:	800 V
rated surge voltage Uimp :	6 kV

SCCR: 35 kA with NZM1 125 A / 480 V AC 

Brand 
Woehner or equivalent

Part No.
32568000A