Text for specification

Description
EQUES®60Classic
busbar adapter 500 A, 4-pole
185 x 300
60Classic

Standards
IEC 61439-1:2011

Approvals
CSA, UL

Electrical data
Rated current (IEC):	500 A
rated voltage (IEC) AC:	690 V

rated current (UL):	630 A
rated voltage (UL) AC:	600 V

rated isolation voltage Ui AC:	800 V
rated surge voltage Uimp :	6 kV

SCCR: 65 kA with 140G-K / 480 V AC, 65 kA with Tmax T5 / 480 V AC 

Brand 
Woehner or equivalent

Part No.
32585000