Text for specification

Description
SECUR 60Classic PowerLiner
busbar mounted switch-disconnector-fuse
for fuses 10x38 IEC 60269-2
63 A / 3P
60Classic

Standards
IEC 60947-1:2020
IEC 60947-3:2020 AC ratings only

Electrical data
rated current (IEC):	32 A
rated voltage (IEC) AC:	690 V
rated voltage (IEC) DC:	110 V

AC-23A (400 V)
AC-22A (690 V) 

power dissipation at full load of the item:	5,3 W

rated isolation voltage Ui AC:	500 V
rated surge voltage Uimp :	6 kV
max. permitted voltage (IEC) AC:	725 V

for fuse links gG and aM as per IEC / EN 60269-2

The function of isolation between incoming and outgoing contacts is provided by the opening of the switching mechanism as required in the standard. 

Brand 
Woehner or equivalent

Part No.
31232000