Text for specification

Description
flexible copper busbar, plain, insulated
6x 32 x 1
715 A, length 2 m
Accessories

Standards
IEC 61439-1:2011

Approvals
UL

Electrical data
Rated current (IEC):	715 A

power dissipation at full load of the item:	134,6 W

Material properties
Insulation:
	temperature withstand up to 105 °C
	self-extinguishing, V0 according to UL 94
	breakdown voltage 20 kV
	stretching 370 %

Miscellaneous 
The laminated Cu busbars considerably reduce the effort of connecting busbars. The bending devices required for solid copper busbars are unnecessary. The 2mm-thick insulation means that no additional covering is required.

Brand 
Woehner or equivalent

Part No.
01282000