Text for specification

Description
busbar support
for drilled flat busbars
185mm-System

Standards
IEC 61439-1:2011

Electrical data
rated voltage (IEC) AC:	690 V

rated isolation voltage Ui AC:	1000 V
rated surge voltage Uimp :	8 kV
max. permitted voltage (IEC) DC:	1500 V

Short-circuit withstand capacity: 	Surge current strength &gt; 100kA at 	Busbar support separation 600mm

Material properties
Main body:
	temperature stability 130°C,
	self-extinguishing in acc. to UL 94, 
	creepage resistance CTI 600,
	halogen-free

Miscellaneous 
Type tested at 600mm busbar support separation and busbar 120 x 10mm with internal screw holes
can also be used as centre support.

Brand 
Woehner or equivalent

Part No.
01742000