Text for specification

Description
neutral conductor 250 A, disconnectable
screw M8 at both sides
120 mm long

Standards
IEC 61439-1:2011

Electrical data
Rated current (IEC):	250 A
rated voltage (IEC) AC:	690 V
rated voltage (IEC) DC:	440 V

power dissipation at full load of the item:	2,9 W
max. permitted voltage (IEC) AC:	800 V
max. permitted voltage (IEC) DC:	800 V

Brand 
Woehner or equivalent

Part No.
03657000