Text for specification

Description
EQUES^®30Compact
busbar adapter 160 A, 4-pole
141 x 160
30Compact 5P

Standards
IEC 61439-1:2011

Electrical data
Rated current (IEC):	160 A
rated voltage (IEC) AC:	690 V

power dissipation at full load of the item:	7,4 W

rated isolation voltage U_i AC:	800 V
rated surge voltage U_imp :	6 kV

Brand 
Woehner or equivalent

Part No.
32640000