Text for specification

Description
EQUES®60Classic
busbar adapter 32 A
for direct starter Siemens S0 with spring terminal connection
45 x 200, with 165 mm long leads AWG 10 (6 mm²)
60Classic

Standards
IEC 61439-1:2011

Approvals
CSA, UL

Electrical data
Rated current (IEC):	32 A
rated voltage (IEC) AC:	690 V

rated current (UL):	32 A
rated voltage (UL) AC:	600 V

power dissipation at full load of the item:	3,2 W

rated isolation voltage Ui AC:	800 V
rated surge voltage Uimp :	6 kV

SCCR: 30 kA with S0 12,5 A / 600 V AC, 65 kA with S0 16 A / 480 V AC, 65 kA with S0 25 A / 480 V AC, 50 kA with S0 32 A / 480 V AC 

Material properties
Conductor insulation: 	temperature-resistant up to 150°C

Miscellaneous 
Conductor ends ultrasonically sealed.
Click mechanism when pushing onto the busbar.

Brand 
Woehner or equivalent

Part No.
32659000