Text for specification

Description
EQUES®30Compact
busbar adapter 25 A
for direct starter Siemens S00 with spring terminal connection
45 x 160, with leads AWG 12 (4 mm²)
30Compact 3P

Standards
IEC 61439-1:2011

Electrical data
Rated current (IEC):	25 A
rated voltage (IEC) AC:	690 V

power dissipation at full load of the item:	2,5 W

rated isolation voltage Ui AC:	800 V
rated surge voltage Uimp :	6 kV

Material properties
Conductor insulation: 	temperature-resistant up to 105 °C

Miscellaneous 
Conductor ends ultrasonically sealed.
Click mechanism when pushing onto the busbar.

Brand 
Woehner or equivalent

Part No.
32693000A