Text for specification

Description
EQUES^®60Classic
busbar adapter 100 A
for circuit breaker ABB MS49x and Siemens Sirius frame size S3, 200 mm long
72 x 200, with leads AWG 4 (25 mm²), with metal plate, top connection to the system
60Classic

Standards
IEC 61439-1:2011

Approvals
CSA, UL

Electrical data
Rated current (IEC):	100 A
rated voltage (IEC) AC:	690 V

rated current (UL):	100 A
rated voltage (UL) AC:	600 V

power dissipation at full load of the item:	7,3 W

rated isolation voltage U_i AC:	800 V
rated surge voltage U_imp :	6 kV

SCCR: 65 kA with MS49x / 480 V AC, 65 kA with S3 / 480 V AC 

Miscellaneous 
Conductor ends ultrasonically sealed.
Click mechanism when pushing onto the busbar.

Brand 
Woehner or equivalent

Part No.
32981000A