Text for specification

Description
centre feed unit 1250 A
for cabinet width 600 mm
centre feed unit

Standards
IEC 61439-1:2011

Approvals
UL

Electrical data
Rated current (IEC):	1.250 A
rated voltage (IEC) AC:	690 V

rated current (UL):	1.200 A
rated voltage (UL) AC:	480 V

power dissipation at full load of the item:	46,4 W

rated isolation voltage Ui AC:	1000 V
rated surge voltage Uimp :	8 kV

rated peak withstand current  Ipk max.:	93 kA

4-pole busbar system, can be retrofitted

Miscellaneous 
Clear construction and undrilled connection technology enable safe and cost-efficient solutions to problems.

Brand 
Woehner or equivalent

Part No.
35007000