Text for specification

Description
BROOME10®CrossBoard
power supply 10 A
400 V AC / 24 V DC, with push-in terminals

Standards
IEC 61010-1:2010
IEC 61010-2-201:2013

Approvals
IEC (CB), UL

Electrical data
rated voltage (IEC) AC:	480 V
rated voltage (UL) AC:	480 V

rated isolation voltage U_i AC:	800 V
rated surge voltage U_imp :	6 kV

2-pole feeding at L1 and L2

Terminal points
f+AE max. 1,5 mm²

Miscellaneous 
direct installation to CrossBoard®
efficiency of 95% permits an intallation width of 45 mm
self-protected at short-circuit with intelligent re-start
no pre-fuse needed
overvoltage capacity up to 6 kV

Brand 
Woehner or equivalent

Part No.
36200000A