Text for specification

Description
AMBUS Panel
holder for cylindrical fuses
14x51 / 1P
50 A / 690 V

Standards
IEC 60947-1:2020
IEC 60947-3:2020 AC ratings only

Approvals
IEC (CB), CSA, UL, CCC

Electrical data
rated current (IEC):	50 A
rated voltage (IEC) AC:	690 V

rated current (UL):	50 A
rated voltage (UL) AC:	600 V
rated voltage (UL) DC:	600 V

power dissipation at full load of the item:	0.9 W

rated isolation voltage Ui AC:	800 V
rated surge voltage Uimp :	6 kV

SCCR:	100 kA

for fuse links as per IEC / EN 60269-2 with permitted rated power dissipations
up to max. 5W for gG/gL 
up to max. 3W for aM

Miscellaneous 
large clamping range
 holder for label

Brand 
Woehner or equivalent

Part No.
31115000