Text for specification

Description
EQUES 60Classic
busbar adapter 250 A
terminals 35 - 120 mm² at top
110 x 320
60Classic

Standards
IEC 61439-1:2020

Approvals
CSA, UL

Electrical data
rated current (IEC):	250 A
rated voltage (IEC) AC:	690 V

rated current (UL):	250 A
rated voltage (UL) AC:	600 V

power dissipation at full load of the item:	34.6 W

rated isolation voltage Ui AC:	800 V
rated surge voltage Uimp :	6 kV
max. permitted voltage (IEC) DC:	800 V

rated peak withstand current  Ipk max.:	55.8 kA

Miscellaneous 
Movable fastening rails with M4 slide nuts for safe mounting of the switching devices.

Brand 
Woehner or equivalent

Part No.
32168000