Text for specification

Description
EQUES®60Classic
busbar adapter 80 A
2 adjustable mounting rails
54 x 200, without leads, with terminals 16 mm², operated from behind
60Classic

Standards
IEC 61439-1:2011

Approvals
CSA, UL

Electrical data
Rated current (IEC):	80 A
rated voltage (IEC) AC:	690 V

rated current (UL):	80 A
rated voltage (UL) AC:	600 V

power dissipation at full load of the item:	9.3 W

rated isolation voltage Ui AC:	800 V
rated surge voltage Uimp :	6 kV
max. permitted voltage (IEC) DC:	800 V

Brand 
Woehner or equivalent

Part No.
32467000