Text for specification

Description
CrossLink®60Classic
spare part busbar adapter 250 A
busbar adapter base
60Classic

Standards
IEC 61439-1:2020

Electrical data
Rated current (IEC):	250 A
rated voltage (IEC) AC:	690 V
rated voltage (IEC) DC:	440 V

power dissipation at full load of the item:	24.8 W

rated isolation voltage Ui AC:	800 V
rated surge voltage Uimp :	6 kV
max. permitted voltage (IEC) AC:	725 V
max. permitted voltage (IEC) DC:	462 V

Brand 
Woehner or equivalent

Part No.
32595000