Text for specification

Description
connecting terminal, front connection
for 3-pole comb-type busbar 35 mm², suitable for NH-fuse-switch-disconnector size 00 with screw connection
25 - 95 mm²
Accessories

Standards
IEC 60947-1:2020
IEC 60947-3:2020 AC ratings only

Electrical data
rated insulation voltage:      800V at pollution degree 2; 690V at pollution degree 3

Conductor connection: Cu 25-95mm² s(r); Cu 35-95mm² s(s); Cu 25-70mm² f+AE

Degree of protection:
IP 20 at front in combination NH-LTS, comb-type busbar and connecting terminal possible.
Degree of protection near terminal depends on installation.

Miscellaneous 
Shock protection:	as per DIN EN 50274/BGV A3

Brand 
Woehner or equivalent

Part No.
33378000