Text for specification

Description
EQUES^®60Classic
busbar adapter 63 A
2 adjustable mounting rails
54 x 260, with leads AWG 8 (10 mm²)
60Classic

Standards
IEC 61439-1:2011

Approvals
CSA, UL

Electrical data
Rated current (IEC):	63 A
rated voltage (IEC) AC:	690 V

rated current (UL):	65 A
rated voltage (UL) AC:	600 V

power dissipation at full load of the item:	6.9 W

rated isolation voltage U_i AC:	800 V
rated surge voltage U_imp :	6 kV

SCCR: 100 kA with MS45x 60 A / 480 V AC , 100 kA with PKZ5 60 A / 480 V AC  

Material properties
Conductor insulation: 	temperature-resistant up to 105 °C

Miscellaneous 
Conductor ends ultrasonically sealed.
Click mechanism when pushing onto the busbar.

Brand 
Woehner or equivalent

Part No.
32461000