Text for specification

Description
CRITO®
terminal for round and sector shaped conductor
95 - 300 mm²
60Classic
100Energy
185mm-System
centre feed unit

Standards
IEC 61439-1:2020
IEC 60999-1:1999
IEC 60999-2:2003

Electrical data
Rated current (IEC):	630 A
rated voltage (IEC) AC:	690 V
current capacity (IEC) max.:	630 A
max. permitted voltage (IEC) AC:	1000 V
max. permitted voltage (IEC) DC:	1500 V

rated peak withstand current  Ipk max.:	81.4 kA

Miscellaneous 
Indication of nominal cross-section and tightening torque marked on the terminal.
Terminal can be subsequently fitted onto and removed from mounted busbar.

Brand 
Woehner or equivalent

Part No.
01094000