Text for specification

Description
CRITO®
profile terminal
320 - 800 mm²
terminal space 41 x 23-45
60Classic
185mm-System
centre feed unit

Standards
IEC 61439-1:2011

Approvals
CSA, UL

Electrical data
Rated current (IEC):	1,600 A
rated voltage (IEC) AC:	690 V

rated current (UL):	1,200 A
rated voltage (UL) AC:	600 V
current carrying capacity for centre feed:	1,600 A
max. permitted voltage (IEC) AC:	1000 V
max. permitted voltage (IEC) DC:	1500 V

rated peak withstand current  Ipk max.:	81.9 kA

SCCR:	25 kA

Terminal points
terminal space 41 x 23-45
1 terminal screw M12

Miscellaneous 
also rigid copper busbars can be connected if they are installed without mechnical tension 

Brand 
Woehner or equivalent

Part No.
01513000