Text for specification

Description
NH busbar mounted fuse base, 250 A
screw
size 1 / 3P
40mm-System

Standards
IEC 60269-1:2006 + A1:2009 + A2:2014
IEC 60269-2:2013 + A1:2016

Electrical data
Rated current (IEC):	250 A
rated voltage (IEC) AC:	690 V
rated voltage (IEC) DC:	440 V

power dissipation at full load of the item:	22.0 W
rated surge voltage Uimp :	6 kV
max. permitted voltage (IEC) AC:	800 V
max. permitted voltage (IEC) DC:	800 V

for fuse links IEC 60269-2 / DIN VDE 0636-201 size 1 up to 32W power dissipation

Brand 
Woehner or equivalent

Part No.
03705000