Text for specification

Description
CAPUS®Panel
changeover switch 3-pole
screw M6
160 A

Standards
IEC 60947-1:2007 + A1:2010 + A2:2014 + A3:2020
IEC 60947-6-1:2021

Electrical data
Rated current (IEC):	160 A
rated voltage (IEC) AC:	690 V

power dissipation at full load of the item:	23.4 W

rated isolation voltage Ui AC:	1000 V
rated surge voltage Uimp :	8 kV
rated making capacity:	10 kA

Gebrauchskategorien siehe Datenblatt (unter Downloads) 

Brand 
Woehner or equivalent

Part No.
23101000AD