Text for specification

Description
EQUES^®CrossBoard
adapter 16 A
1 fixed mounting rail, with fuse-carrier 10x38 / Class CC
22.5 x 160, with leads AWG 14 (2.5 mm²)

Standards
IEC 61439-1:2011

Approvals
IEC (CB), UL

Electrical data
Rated current (IEC):	16 A
rated voltage (IEC) AC:	690 V

rated current (UL):	12.5 A
rated voltage (UL) AC:	600 V

power dissipation at full load of the item:	4.0 W

rated isolation voltage U_i AC:	800 V
rated surge voltage U_imp :	6 kV
max. permitted voltage (IEC) AC:	725 V

Miscellaneous 
Leitungsenden ultraschallverdichtet.

Brand 
Woehner or equivalent

Part No.
36009000A