Text for specification

Description
MOTUS®60Classic
hybrid motor starter, 3-pole
direct and reversing starter 0.18 - 3.0 A / switch for resistive loads 0.18 - 3.0 A
with IO-Link interface
60Classic

Standards
IEC 60947-1:2007 + A1:2010 + A2:2014
IEC 60947-4-2:2011
IEC 61508-1:2010
ISO 13849-1:2015

Approvals
UL

Electrical data
Rated current (IEC):	3 A
rated voltage (IEC) AC:	500 V

rated current (UL):	3 A
rated voltage (UL) AC:	500 V

power dissipation at full load of the item:	6.0 W

rated isolation voltage Ui AC:	550 V
rated surge voltage Uimp :	6 kV

SCCR: 100 kA with JDDZ fuse Class J 400 A / 600 V AC  

Terminal points
Screw terminals (solid round, flexible, flexible with wire-end ferrule) 
0.14 - 2.5mm² / 0.5 - 0.6Nm
The cable outlet is provided with a pluggable terminal

Miscellaneous 
4 functions integrated:
Right contactor
Left contactor
Motor protection relay

Installed width only 22.5mm
30 million electrical switching operations

Brand 
Woehner or equivalent

Part No.
36125000A