Text for specification

Description
busbar support, lateral
centre feed unit

Standards
IEC 61439-1:2011

Approvals
UL

Electrical data
rated voltage (IEC) AC:	690 V
rated voltage (UL) AC:	600 V

rated isolation voltage U_i AC:	1000 V
rated surge voltage U_imp :	8 kV

can also be used for 4-pole busbar systems

Material properties
Main body:
	temperature stability 130°C,
	self-extinguishing in acc. to UL 94, 
	creepage resistance CTI 600,
	halogen-free

Brand 
Woehner or equivalent

Part No.
35008000