Text for specification - draft 

Description
CAPUS®Panel
switch-disconnector 2-pole
screw M10, without handle
400 A

Standards
IEC 60947-1:2020
IEC 60947-3:2020

Approvals
IEC (CB), VDE

Electrical data
Rated current (IEC):	400 A
rated voltage (IEC) DC:	1500 V

power dissipation at full load of the item:	11.0 W
current capacity (IEC) max.:	400 A
rated surge voltage Uimp :	12 kV
max. permitted voltage (IEC) DC:	1500 V

Gebrauchskategorien siehe Datenblatt (unter Downloads) 

Brand 
Woehner or equivalent

Part No.
23053000AD