Text for specification

Description
AMBUS®Panel
holder for cylindrical fuses
Class J / 3P, box terminal 50 mm²
30 A / 600 V (21x57)

Standards
IEC 60269-1:2006 + A1:2009 + A2:2014
IEC 60269-2:2013 + A1:2016, Fuse system H

Approvals
CSA, UL

Electrical data

rated current (UL):	30 A
rated voltage (UL) AC:	600 V
rated voltage (UL) DC:	600 V

power dissipation at full load of the item:	0.6 W

SCCR:	200 kA

for Class J fuses 1 - 30A as per UL 248-8 (21x57)

Miscellaneous 
large clamping range, also for two identical conductors (adjacent)
holder for label

Brand 
Woehner or equivalent

Part No.
31287000