Text for specification

Description
EQUES^®60Classic
busbar adapter 160 A, 3-pole
90 x 200
60Classic

Standards
IEC 61439-1:2011

Approvals
CSA, UL

Electrical data
Rated current (IEC):	160 A
rated voltage (IEC) AC:	690 V

rated current (UL):	160 A
rated voltage (UL) AC:	600 V

power dissipation at full load of the item:	12.0 W

rated isolation voltage U_i AC:	800 V
rated surge voltage U_imp :	6 kV

Brand 
Woehner or equivalent

Part No.
32577000