Text for specification

Description
CrossLink^®60Classic
busbar adapter base 125 A
busbar adapter base
49.5 mm x 200 mm, only for use with QU-NH000
60Classic

Standards
IEC 61439-1:2011

Electrical data
Rated current (IEC):	125 A
rated voltage (IEC) AC:	690 V

power dissipation at full load of the item:	4.0 W

rated isolation voltage U_i AC:	800 V
rated surge voltage U_imp :	6 kV

Brand 
Woehner or equivalent

Part No.
32620000A