Text for specification

Description
QUADRON®60Classic
bus mounted fuse holder Class J
for fuse links Class J 225 - 400 A (54x181)
3P, with box terminal
60Classic

Standards
IEC 60269-1:2006 + A1:2009 + A2:2014
IEC 60269-2:2013 + A1:2016, Fuse system H

Approvals
CSA, UL

Electrical data

rated current (UL):	400 A
rated voltage (UL) AC:	600 V
rated voltage (UL) DC:	600 V

power dissipation at full load of the item:	46.8 W

SCCR:	65 kA

Terminal points
tunnel terminal with hole of 23,0 mm diameter

acc. to IEC / EN :
16 - 240 (300) mm²
flexible cables, directly or with wire-end ferrule, 
solid and stranded round cables, 
Md 38 - 40 Nm

(flexible cables of maximum cross-section may not fit when using wire-end ferrule)

acc. to UL :
AWG 4 - MCM 600
stranded cables Class B acc. to UL 486E
336 - 355 lb.in.

Miscellaneous 
the product is based on the UL approval in category IZLT2 also listed in category NMTR (file E123577)

Brand 
Woehner or equivalent

Part No.
33311000