Text for specification

Description
connection busbar support
3-pole, with integrated terminals 1.5 - 16 mm²
60Classic

Standards
IEC 61439-1:2011

Electrical data
Rated current (IEC):	63 A
rated voltage (IEC) AC:	690 V

power dissipation at full load of the item:	0.8 W
current capacity (IEC) max.:	80 A

rated isolation voltage Ui AC:	800 V
rated surge voltage Uimp :	6 kV

Current capacity of the clamping point 80A
short-circuit withstand rating:
surge current strength &gt; 30kA at busbar support separation of 550mm
surge current strength &gt; 50kA at busbar support separation of 250mm
further values in the short-circuit withstand rating diagram

Material properties
Main body:
	temperature stability 125°C, 
	self-extinguishing in acc. to UL 94, 
	creepage resistance CTI 600,
	halogen-free
Screws:
	screw +/- (PZ2), galvanized, chromized 
Handle:
	temperature stability 125°C, 
	self-extinguishing in acc. to UL 94,
	creepage resistance CTI 600

Miscellaneous 
Connection busbar support with integrated terminals for feeding or tapping the busbar
with internal screw holes, can also be used as centre support.

Brand 
Woehner or equivalent

Part No.
01484000