Text for specification

Description
universal busbar support
3-pole with additional external screw holes
60Classic

Standards
IEC 61439-1:2011

Electrical data
rated voltage (IEC) AC:	800 V

rated isolation voltage Ui AC:	1000 V
rated surge voltage Uimp :	8 kV
max. permitted voltage (IEC) DC:	1500 V

rated peak withstand current  Ipk max.:	73 kA

Miscellaneous 
With additional external screw holes
can also be used as centre support

Brand 
Woehner or equivalent

Part No.
01500000