Text for specification

Description
CAPUS^®Panel
switch-disconnector 3-pole
screw M12, graphite-grey handle
3150 A

Standards
IEC 60947-1:2020
IEC 60947-3:2020 AC ratings only

Approvals
CCC

Electrical data
Rated current (IEC):	3,150 A
rated voltage (IEC) AC:	500 V

power dissipation at full load of the item:	595.2 W

rated isolation voltage U_i AC:	1000 V
rated surge voltage U_imp :	12 kV
rated making capacity:	110 kA

Gebrauchskategorien siehe Datenblatt (unter Downloads) 

Brand 
Woehner or equivalent

Part No.
23010000AD