Text for specification

Description
busbar support 3 phases + N + E
Accessories

Standards
IEC 61439-1:2011

Electrical data
rated voltage (IEC) AC:	690 V

rated isolation voltage Ui AC:	800 V
rated surge voltage Uimp :	6 kV

short-circuit capacity :
Ipk = min. 35 kA (2 busbar supports in 250 mm distance)

Material properties
Main body:
	temperature stability 125°C, 
	self-extinguishing in acc. to UL 94, 
	creepage resistance CTI 600,
	halogen-free
Screws:
	screw +/- (PZ2), galvanized, chromized 

Brand 
Woehner or equivalent

Part No.
01138000