Text for specification

Description
CAPUS®Panel
switch-disconnector 3-pole
screw M10, graphite-grey handle
400 A

Standards
IEC 60947-1:2020
IEC 60947-3:2020 AC ratings only

Approvals
CCC

Electrical data
Rated current (IEC):	400 A
rated voltage (IEC) AC:	690 V

power dissipation at full load of the item:	38.4 W

rated isolation voltage Ui AC:	1000 V
rated surge voltage Uimp :	8 kV
rated making capacity:	26.5 kA

Gebrauchskategorien siehe Datenblatt (unter Downloads) 

Brand 
Woehner or equivalent

Part No.
23004000AD