Text for specification

Description
EQUES^®60Classic
busbar adapter 25 A 
for direct starter Eaton PKZM01, PKE12
45 x 200, with leads AWG 12 (4 mm²)
60Classic

Standards
IEC 61439-1:2011

Approvals
CSA, UL

Electrical data
Rated current (IEC):	25 A
rated voltage (IEC) AC:	690 V

rated current (UL):	25 A
rated voltage (UL) AC:	600 V

power dissipation at full load of the item:	1.9 W

rated isolation voltage U_i AC:	800 V
rated surge voltage U_imp :	6 kV

SCCR: 30 kA with PKZM0 12,5 A / 600 V AC, 65 kA with PKZM0 16 A / 480 V AC, 65 kA with PKZM0 25 A / 480 V AC, 50 kA with PKZM0 32 A / 480 V AC 

Miscellaneous 
Conductor ends ultrasonically sealed.
Click mechanism when pushing onto the busbar.

Brand 
Woehner or equivalent

Part No.
32450000