Text for specification

Description
EQUES®60Classic
busbar adapter 16 A
for direct starter Allen-Bradley 140M-RC2E, Eaton PKZM0, Siemens S00, Schneider Electric GV2 with spring terminals
45 x 200, with leads AWG 14 (2.5 mm²)
60Classic

Standards
IEC 61439-1:2011

Approvals
CSA, UL

Electrical data
Rated current (IEC):	16 A
rated voltage (IEC) AC:	690 V

rated current (UL):	12 A
rated voltage (UL) AC:	600 V

power dissipation at full load of the item:	0.8 W

rated isolation voltage Ui AC:	800 V
rated surge voltage Uimp :	6 kV

Miscellaneous 
Conductor ends ultrasonically sealed.
Click mechanism when pushing onto the busbar.
For switching devices with spring-loaded terminals

Brand 
Woehner or equivalent

Part No.
32429000