Text for specification

Description
EQUES®CrossBoard
adapter 32 A
1 fixed mounting rail, with leads AWG 10 (6 mm²)
45 x 160

Standards
IEC 61439-1:2020

Approvals
IEC (CB), UL

Electrical data
Rated current (IEC):	32 A
rated voltage (IEC) AC:	690 V

rated current (UL):	30 A
rated voltage (UL) AC:	600 V

power dissipation at full load of the item:	2.1 W

rated isolation voltage Ui AC:	800 V
rated surge voltage Uimp :	6 kV

SCCR: 65 kA with any NKJH/7 Comb. Motor Controller 32 A / 480 V AC 

Miscellaneous 
Conductor ends ultrasonic compressed.
Click mechanism when pushing onto the CrossBoard®.

Brand 
Woehner or equivalent

Part No.
32682000A