Text for specification

Description
QUADRON^®60Classic
busbar mounted fuse holder Class J
for fuse links Class J 1 - 30 A (21x57)
3P, with box terminal
60Classic

Standards
IEC 60269-1:2006 + A1:2009 + A2:2014
IEC 60269-2:2013 + A1:2016, Fuse system H

Approvals
UL

Electrical data

rated current (UL):	30 A
rated voltage (UL) AC:	600 V
rated voltage (UL) DC:	600 V

power dissipation at full load of the item:	2.1 W

SCCR:	200 kA

System component: degree of protection IP30 at front as per DIN EN 60529, degree of protection near terminal depends on installation
adapter module: front side degree of protection IP20 as per DIN EN 60529 (finger-safe)

Terminal points
AWG 12 - AWG 2/0 stranded, equivalent 3,3 - 67,4 mm²
AWG 14 - AWG 10 solid, equivalent 215 - 5,3 mm²

Miscellaneous 
the product is based on the UL approval in category IZLT2 also listed in category NMTR (file E123577)

CrossLink® adapter technology
Fast and safe conversion of the connection for top or bottom; the parts under voltage remain shock protected
Simple and safe clicking into place and making contact
Safe connection through shock protection split into two
Busbar supports for flat busbars can be mounted above each other

Brand 
Woehner or equivalent

Part No.
33421000